Control System

Light

Sensor (Photo résistor)

(1) (2) (3)

User

1. Presence or not of the User
2. Informations from the sensor detecting if the user is present or not
3. Actions by the controller depending on the received informations.